Real-time PAA Disinfection Control in Municipal Wastewater Treament

Kate Newhart

11/13/2019

# October 2018 Evaluation

Need inf flow to calculate HRT

NN Models were built to predict PAA at the “1-min” and “1/2 basin” sample point to predict C1 and C2

# July 2019 Evaluation

Change from PAA setpoint to actual flow-paced concentraiton?



